Altavoces coaxiales

BP215MCX new



BP215MCX
Features:
· 1500 W RMS
· 3-way Triaxial System
· Frequency response - 80Hz-22kHz
· Three-amplified operation
· Designed for PA, fixed installation and touring.
The band pass design combined with two highly efficient 15" transducers produces an efficiency of 104 dB at 1 W / 1 m. A power rating of 1100 W RMS enables a sustained output of 134 dB to be maintained.


MCX115-1.5 new


Features:
· Single point source system providing coherent wave front           
· 15”/1.5” coaxial  loudspeaker
· High power handling of 800w AES
· 70° conical Constant Directivity Coverage Horn
· Passive or bi-amp operation
· Designed for both: PA, stage monitoring and touring
 
 MCX115-2.0 new


[bookmark: _GoBack]Features:
· Triaxial point source system providing coherent wave front           
· 15”/2” Coaxial  loudspeaker
· High power handling of 880w
· 60° conical Constant Directivity Coverage Horn
· Superb quality sound
· Designed for both:  PA and stage monitoring

TCX118 new



Features:
· Single point source system providing coherent wave front           
· 18”/2” coaxial  loudspeaker
· High power handling of 1000w
· 90° x 40° Constant Directivity Coverage Horn
· Superb quality sound
· Designed for both: PA
The Clear Sound  TCX118 is a full range 3-way Triaxial  loudspeaker system that features a high power 18" cone driver and a 2" coaxial  driver coupled to a 90° x 40° waveguide. As a three way system, the TCX118 may be driven passively or with bi-amplification to provide extremely high acoustic output. 

