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BP215MCX new



BP215MCX
Features:
· 1500 W RMS
· 3-way Triaxial System
· Frequency response - 80Hz-22kHz
· Three-amplified operation
· Designed for PA, fixed installation and touring.
The band pass design combined with two highly efficient 15" transducers produces an efficiency of 104 dB at 1 W / 1 m. A power rating of 1100 W RMS enables a sustained output of 134 dB to be maintained.


MCX115-1.5 new


Features:
· Single point source system providing coherent wave front           
· 15”/1.5” coaxial  loudspeaker
· High power handling of 800w AES
· 70° conical Constant Directivity Coverage Horn
· Passive or bi-amp operation
· Designed for both: PA, stage monitoring and touring
 
 MCX115-2.0 new



Features:
· Triaxial point source system providing coherent wave front           
· 15”/2” Coaxial  loudspeaker
· High power handling of 880w
· 60° conical Constant Directivity Coverage Horn
· Superb quality sound
· Designed for both:  PA and stage monitoring

TCX118 new



Features:
· Single point source system providing coherent wave front           
· 18”/2” coaxial  loudspeaker
· High power handling of 1000w
· 90° x 40° Constant Directivity Coverage Horn
· Superb quality sound
· Designed for both: PA
The Clear Sound  TCX118 is a full range 3-way Triaxial  loudspeaker system that features a high power 18" cone driver and a 2" coaxial  driver coupled to a 90° x 40° waveguide. As a three way system, the TCX118 may be driven passively or with bi-amplification to provide extremely high acoustic output. 
. 














INSTALACIÓN FIJA

CF 08



Features:
 
· 2-way compact versatile full range system
· High power handling of 300 W
· 1"  compression driver
 
CF 110

· 2-way  full range
· 400 W RMS

CF 110 is an exceptionally high-output full range system, suitable for premises with limited space and low-rise ceiling (pubs, restaurants, discotheques and night clubs). The system contains one 10" SD cone driver and 1" BMS high frequency driver.


CF 112


· 2-way  full range
· 550 W RMS

CF 112 is an exceptionally high-output full range system, suitable for premises with limited space and low-rise ceiling (pubs, restaurants, discotheques and night clubs). The system contains one 12" SD cone driver and 1" BMS high frequency driver.

CF 1510



· 3-way  full range
· 1000W RMS

CF 1510 is an exceptionally high-output full range system, suitable for premises with limited space and low-rise ceiling (pubs, restaurants, discotheques and night clubs). The system contains one 15" SD cone driver, one 10" SD mid-bass cone driver and 1" BMS high frequency driver.

CF 215W

Features:
· 3-way  full range
· 2000W RMS
· Bi-amplified operation
· Designed for fixed installation

CF 215W is full range system, suitable for premises with limited space where it is not possible to put subwoofers on the ground. The system contains two 15" SD cone drivers, one 10" SD mid-bass cone driver and 1" BMS high frequency driver.
CLR 208


Features:
· 500W rms
· 2-way  full range
· Passive or bi-amplified operation
· Designed for fixed installation and touring
CLR 208  is very suitable for small clubs and piano bars. It contains two 8" SD cone drivers and two 1" BMS high frequency drivers. It is very good choice because of its 180° coverage.

CLR 312


Features:
· 2-way  full range system
· Very high SPL from 80-Hz-22kHz
· 120° multihorn
· bi-amp operation
· Designed for fixed installation

CLR 408


· 1000W rms
· 2 - way full range
 
CLR 408 is very suitable for clubs where the interior does not allow any speakers to be put on the walls. It contains four 8" SD cone drivers and four 1" BMS high frequency drivers. CLR is an excellent choice because of its 360° coverage.

CLR 612

3000 W  2-way  bi-amp operation
Features:
· 2-way  full range system
· Very high SPL from 70Hz-22kHz
· 240° multihorn
· bi-amp operation
· Designed for fixed installation

CLR 815

Features:
· 3-way  full range system
· Very high SPL from 33-Hz-22kHz
· 360° coverage
· bi-amp operation
· Designed for fixed installation

MONITORES DE ESTUDIO
KS 105


Features:
KS 105 is a compact speaker, suitable for small clubs and also for homes. It is an excellent choice for everyone who loves Hi-Fi sounding!

KS 205

Features:
KS 205 is a compact speaker, suitable for small clubs and also for homes. It is an excellent choice for everyone who loves Hi-Fi sounding!



Monitores

MCX115-2 new

3-way full range-Triaxial
Features:
· Single point source system providing coherent wave front
· 15”/2” Triaxial  loudspeaker
· High power handling of 1000w
· 70° conical Constant Directivity Coverage Horn
· Superb quality sound
· Designed for both:  stage monitoring


MS 112

Features:
· 2-way compact versatile full range system
· High power handling of 550 W
· 90° x 75° Constant Directivity Coverage Horn
· Designed for both: PA and stage monitoring
The MS 112 is a versatile, full range two-way loudspeaker system that features a high power SD-12" woofer and a 1" compression

MS 115

2-way full range
Features:
· 2-way compact versatile full range system
· High power handling of 550 W
· 90° x 75° Constant Directivity Coverage Horn
· Designed for both: PA and stage monitoring
The MS 115 is a versatile, full range two-way loudspeaker system that features a high power SD-15" woofer and a 1"  compression driver. 

POINT SOURCE
BP1508 new

Features:
· 1500 W RMS
· 3-way  Coaxial Band-pass and Horn Loaded  system
· Frequency response - 80Hz-22kHz
· Three-amplified operation
· Designed for PA, fixed installation and touring.
The band pass design combined with two highly efficient 15" transducers produces an efficiency of 104 dB at 1 W / 1 m. A power rating of 1100 W RMS enables a sustained output of 134 dB to be maintained.

HL 212H2


TRIAXIAL HORN LOADED CONCERT SYSTEM

Features:
· 3-way on-axis horn loaded point source loudspeaker system
· Revolutionary 2" Coaxial Compression Driver
· Precise directivity
· Very high SPL (144 dB peak)
 

HL1508 new


Features:
· 3-way  full range system
· High Efficiency Horn Loaded design
· Very high SPL from 100Hz-20kHz 
· Three-amplified or Two-aplified operation 
· Designed for horizontal array and installation

The horn loaded design combined with one highly efficient 15" transducers produces an efficiency of 103 dB at 1 W / 1 m. A power rating of 800 W RMS enables a sustained output of 132 dB to be maintained.








HL1582 new



Features:
· 3-way  full range system
· High Efficiency Horn Loaded design
· Very high SPL from 100Hz-20kHz 
· Three-amplified or Two-amplified operation 
· Designed for touring and verical installation
 The mid and high sections are loaded by a wave converter which transforms the spherical waves into cylindrical isophase waves.
The horn loaded design combined with one highly efficient 15" transducers produces an efficiency of 103 dB at 1 W / 1 m. A power rating of 600 W RMS enables a sustained output of 132 dB to be maintained.












LINE ARRAYS

LA 2108H1 new

Features:
· Two 1" neodymium  drivers
· Two 8" mid range driver
· Two 10" ultra low distortion woofer
· 90° horizontal coverage
· Variable curving 0° to 10°
· Outstanding SPL capacity at very low power compression
· Highest output to size ratio
· Highest output to weight ratio
· Superior sound
· In the mid section (8'' speaker) there is an option to be used specially selected according to T&S parameters FERROFLUID which benefits are:

Increased thermal power handling
Reduced thermal power compression
Smoothing of frequency response curve
Reduced distortion
Reduced warranty returns
Increased production yields

 The presence of horns leads to an extremely high sound pressure, low distortions and an optimal sound dispersion.

 In order to achieve a flat wave in the high-frequency spectrum we use two 1'' drivers.

 The high sections are loaded by a wave converter which transforms the spherical waves into cylindrical isophase waves.
 In this way the interference between them is reduced to minimum and as a result there is maximum concentration in mid- and high-frequency spectrum.

 An exceptional Hi-Fi sound with incredible sound pressure and phase characteristics is achieved.

 In combination with BP218LF and HL118, the system is a perfect choice for sports halls and stadiums.

The loudspeaker shall be operated with a separate dedicated
electronic controller.

LA V3-LCS
 
Features:
· 2000 Watt Rms
· Four 1'' neodymium drivers
· Two 8" mid range drivers
· Two 10" ultra low distortion woofers
· 90° horizontal coverage
· Variable curving 0° to 10°
· Outstanding SPL capacity at very low power compression
· Highest output to size ratio
· Highest output to weight ratio
· Superior sound
 LA V3-LCS can be manufactured to work with a liquid cooling system in order to reduce the heat in each one of the speakers, which allows the system to work for a long time without any change in the sound pressure level. In the mid section (8'' loudspeaker) there is an option to be used specially selected according to T&S parameters FERROFLUID which benefits are:

· Increased thermal power handling
· Reduced thermal power compression
· Smoothing of frequency response curve
· Reduced distortion
· Reduced warranty returns
· Increased production yields

The presence of horns leads to an extremely high sound pressure, low distortions and an optimal sound dispersion.
 In order to achieve a flat wave in the mid-frequency and in the high-frequency
spectrum we use two 8'' speaker and four 1'' drivers.
 The mid and high sections are loaded by a wave converter which transforms the spherical waves into cylindrical isophase waves.
 In this way the interference between them is reduced to minimum and as a result there is maximum
concentration in mid- and high-frequency spectrum.
 An exceptional Hi-Fi sound with incredible sound pressure and phase characteristics is achieved.
 In combination with RLH 118 SX or HL121, the system is a perfect choice for sports halls and stadiums.
The loudspeaker shall be operated with a separate dedicated
electronic controller.


V3-LCS mini new



Features:
· Two 1" neodymium planar wave drivers
· One 8" mid range driver
· One 10" ultra low distortion woofer
· 90° horizontal coverage
· Variable curving 0° to 10°
· Outstanding SPL capacity at very low power compression
· Highest output to size ratio
· Highest output to weight ratio
· Superior sound
· In every speaker there is an option to be used specially selected according to T&S parameters FERROFLUID which benefits are:

Increased thermal power handling
Reduced thermal power compression
Smoothing of frequency response curve
Reduced distortion
Reduced warranty returns
Increased production yields

 The presence of horns leads to an extremely high sound pressure, low distortions and an optimal sound dispersion.

 In order to achieve a flat wave in the mid-frequency and in the high-frequency spectrum we use one 8'' speaker and two 1'' drivers.

 The mid and high sections are loaded by a wave converter which transforms the spherical waves into cylindrical isophase waves.

 In this way the interference between them is reduced to minimum and as a result there is maximum concentration in mid- and high-frequency spectrum.

 An exceptional Hi-Fi sound with incredible sound pressure and phase characteristics is achieved.

 In combination with HL121, the system is a perfect choice for sports halls and stadiums.

The loudspeaker shall be operated with a separate dedicated
electronic controller.
 
SERIE TOURING

TS 08 new

2-way coaxial full range
Features:
 
· Extreme compact multidesign enclosure
· High power handling of 300 W
· 1"  compression driver
· For both touring and installation
 
The  TS08 is  a  compact  versatile  full  range 2-way coaxial loudspeaker system that features an 8” ultra low distortion.  Low  frequency  driver  and  a  1” compression  driver coupled to a 90° conical wood waveguide.

TS 212H2 new

TS212H2
 
· 3-way compact full range system
· Very high power rating of 1200W
· Unique 2" coaxial driver
· Double 12" ultra low distortion woofers
· Passive or bi-amplified operation
· Designed for fixed installation and touring
The TS212H2 is an extremely high output 3-way full range system engineered to deliver high fidelity sound in medium to long throw applications. The unique 2” coaxial driver mounted on a 90° x 40° waveguide produces an unparalleled clean mid / high range above 800 Hz. The double high power 12”  woofer provide powerful and extended low frequency response with immense headroom.
TS 215H2 new

TS 215H2
3-way full range multidesign
Features:
· 3-way  full range system
· Designed for applications requiring more SPL and bass than single TS Series speakers.
· Very high power of 1800W
· 2" coaxial  driver
· Double SD-15" ultra low distortion woofers
· Passive or bi-amplified operation
· Designed for fixed installation and touring













SUBWOOFER
BP 218


 2000 Wrms Bandpass Parallel Double -Tuned Box with 2 x 18'' loudspeakers characterized with maximum output power. BP218 is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion. It is perfect for house, techno, live music!
Features:
· SD-2x18" high excursion woofer.
· Low power compression, superb quality sound
· Very high power of 2000 Wrms
BP118LF  

1000 W Bandpass Parallel Double -Tuned Box with 1 x 18'' loudspeakers.
An excellent transient response produces fast high impact bass that is able to reproduce detailed and accurate low frequency details. The band-pass design is combined with one highly efficient 18” loudspeaker which produces an efficiency of 102dB at 2.83V/1m. A power rating of 1000Wrms enables a sustained output of 132dB to be maintained.
BP18LF is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion. It is perfect for Drum and Bass, House, Techno, Live music!

BP218LF

 2000 Wrms Bandpass Parallel Double -Tuned Box with 2 x 18'' loudspeakers.
An excellent transient response produces fast high impact bass that is able to reproduce detailed and accurate low frequency details. The band-pass design is combined with two highly efficient 18” loudspeakers which produces an efficiency of 104dB at 1W/1m. A power rating of 2000Wrms enables a sustained output of 136dB to be maintained.
BP218LF is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion. It is perfect for Drum and Bass, House, Techno, Live music!


HL 118

 
 1000 Wrms Horn-loaded subwoofer with one 18'' speaker characterized with maximum low-frequency output power. HL 118 is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion.
Features:
· SD-18" high excursion woofer
· Low power compression, superb quality sound
· Very high power of 1000 Wrms
HL 118 BR new

Description
Very high output Horn/Reflex
loaded sub-woofer
· 2000Wrms
· Horn and Reflex Loaded Subwoofer
· 18" ultra-long excursion high power bass driver
· 8 ohm nominal impedance
· Frequency response 35Hz-200Hz / -3dB one enclosure (29Hz-200Hz /-3dB four enclosure)

HL 118 SX

2000 Wrms Horn-loaded subwoofer with one 18'' speaker characterized with maximum low-frequency output power. HL 118 -SX  is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion.
Features:
· SD-18" high excursion woofer
· Low power compression, superb quality sound
· Very high power of 2000 Wrms
 
HL 121 new

2000 W Horn-loaded subwoofer with one 21'' speaker characterized with maximum low-frequency output power. HL 121 is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion. It is perfect for drum'n'bass!
Features:
 
· SD-21" high excursion woofer.
· Low power compression, superb quality sound
· Very high power of 2000 W
 

HL 212 BR new

Features:
· 1600Wrms
· Horn and Reflex Loaded Mid Bass
· 2x12" ultra-long excursion high power bass driver
· 4 ohm nominal impedance
· Frequency response 75Hz-350Hz/-3dB
This Horn and Reflex Loaded Mid Bass device delivers punchy, well defined upper-bass and low-mid frequencies.

HL 212 MB

Features:
· 1600Wrms
· Horn Loaded Mid Bass
· 2x12" high power bass driver
· 4 ohm nominal impedance
· Frequency response 105Hz-800Hz/-3dB
This Horn Loaded Mid Bass device delivers punchy, well defined upper-bass and mid frequencies.

PW 112 new

600 W passive subwoofer
Features:
· SD-12"  ultra low distortion woofer.
· Low power compression, superb quality sound
PW 115

1000 W Passive subwoofer
Features:
· SD-15" high excursion woofer
· Low power compression, superb quality sound
· Very high power of 1000 Wrms

PW 118

1000 W Passive subwoofer
Features
· SD-18" high excursion woofer
· Low power compression, superb quality sound
· Very high power of 1000 W
PW 215

2000 W Passive subwoofer
Features:
· Double  SD-15" high excursion woofer
· Low power compression, superb quality sound
· Very high power of 2000 Wrms
PW 218

2000 W Passive subwoofer
Features:
· Double  SD-18" high excursion woofer
· Low power compression, superb quality sound
· Very high power of 2000 Wrms

RLH 118 SX new

2000 Wrms  Rear-loaded horn subwoofer with one SD 18BX127 speaker characterized with maximum low-frequency output power. RLH 118 SX  is the optimal decision for sports halls and stadiums because of its high SPL and bass dispersion. It is perfect for drum'n'bass!
Features:
· SD-18BX127 high excursion woofer
· Low power compression, superb quality sound
· Very high power of 2000 Wrms




