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CF 08



Features:
 
· 2-way compact versatile full range system
· High power handling of 300 W
· 1"  compression driver
 
CF 110

· 2-way  full range
· 400 W RMS

CF 110 is an exceptionally high-output full range system, suitable for premises with limited space and low-rise ceiling (pubs, restaurants, discotheques and night clubs). The system contains one 10" SD cone driver and 1" BMS high frequency driver.
CF 112


· 2-way  full range
· 550 W RMS

CF 112 is an exceptionally high-output full range system, suitable for premises with limited space and low-rise ceiling (pubs, restaurants, discotheques and night clubs). The system contains one 12" SD cone driver and 1" BMS high frequency driver.

CF 1510



· 3-way  full range
· 1000W RMS

CF 1510 is an exceptionally high-output full range system, suitable for premises with limited space and low-rise ceiling (pubs, restaurants, discotheques and night clubs). The system contains one 15" SD cone driver, one 10" SD mid-bass cone driver and 1" BMS high frequency driver.

CF 215W

Features:
· 3-way  full range
· 2000W RMS
· Bi-amplified operation
· Designed for fixed installation

CF 215W is full range system, suitable for premises with limited space where it is not possible to put subwoofers on the ground. The system contains two 15" SD cone drivers, one 10" SD mid-bass cone driver and 1" BMS high frequency driver.













CLR 208


Features:
· 500W rms
· 2-way  full range
· Passive or bi-amplified operation
· Designed for fixed installation and touring
CLR 208  is very suitable for small clubs and piano bars. It contains two 8" SD cone drivers and two 1" BMS high frequency drivers. It is very good choice because of its 180° coverage.
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CLR 312


Features:
· 2-way  full range system
· Very high SPL from 80-Hz-22kHz
· 120° multihorn
· bi-amp operation
· Designed for fixed installation

CLR 408


· 1000W rms
· 2 - way full range
 
CLR 408 is very suitable for clubs where the interior does not allow any speakers to be put on the walls. It contains four 8" SD cone drivers and four 1" BMS high frequency drivers. CLR is an excellent choice because of its 360° coverage.

CLR 612

3000 W  2-way  bi-amp operation
Features:
· 2-way  full range system
· Very high SPL from 70Hz-22kHz
· 240° multihorn
· bi-amp operation
· Designed for fixed installation

CLR 815

Features:
· 3-way  full range system
· Very high SPL from 33-Hz-22kHz
· 360° coverage
· bi-amp operation
· Designed for fixed installation

