POINT SOURCE
BP1508 new

Features:
· 1500 W RMS
· 3-way  Coaxial Band-pass and Horn Loaded  system
· Frequency response - 80Hz-22kHz
· Three-amplified operation
· Designed for PA, fixed installation and touring.
The band pass design combined with two highly efficient 15" transducers produces an efficiency of 104 dB at 1 W / 1 m. A power rating of 1100 W RMS enables a sustained output of 134 dB to be maintained.

HL 212H2


TRIAXIAL HORN LOADED CONCERT SYSTEM

Features:
· 3-way on-axis horn loaded point source loudspeaker system
· Revolutionary 2" Coaxial Compression Driver
· Precise directivity
· Very high SPL (144 dB peak)
 

HL1508 new


Features:
· 3-way  full range system
· High Efficiency Horn Loaded design
· Very high SPL from 100Hz-20kHz 
· Three-amplified or Two-aplified operation 
· Designed for horizontal array and installation

The horn loaded design combined with one highly efficient 15" transducers produces an efficiency of 103 dB at 1 W / 1 m. A power rating of 800 W RMS enables a sustained output of 132 dB to be maintained.








HL1582 new



Features:
· 3-way  full range system
· High Efficiency Horn Loaded design
· Very high SPL from 100Hz-20kHz 
· Three-amplified or Two-amplified operation 
· Designed for touring and verical installation
 The mid and high sections are loaded by a wave converter which transforms the spherical waves into cylindrical isophase waves.
The horn loaded design combined with one highly efficient 15" transducers produces an efficiency of 103 dB at 1 W / 1 m. A power rating of 600 W RMS enables a sustained output of 132 dB to be maintained.
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