SERIE TOURING

TS 08 new

2-way coaxial full range
Features:
 
1. Extreme compact multidesign enclosure
1. High power handling of 300 W
1. 1"  compression driver
1. For both touring and installation
 
The  TS08 is  a  compact  versatile  full  range 2-way coaxial loudspeaker system that features an 8” ultra low distortion.  Low  frequency  driver  and  a  1” compression  driver coupled to a 90° conical wood waveguide.

TS 212H2 new

TS212H2
 
1. 3-way compact full range system
1. Very high power rating of 1200W
1. Unique 2" coaxial driver
1. Double 12" ultra low distortion woofers
1. Passive or bi-amplified operation
1. Designed for fixed installation and touring
The TS212H2 is an extremely high output 3-way full range system engineered to deliver high fidelity sound in medium to long throw applications. The unique 2” coaxial driver mounted on a 90° x 40° waveguide produces an unparalleled clean mid / high range above 800 Hz. The double high power 12”  woofer provide powerful and extended low frequency response with immense headroom.
TS 215H2 new

TS 215H2
3-way full range multidesign
Features:
1. 3-way  full range system
1. Designed for applications requiring more SPL and bass than single TS Series speakers.
1. Very high power of 1800W
1. 2" coaxial  driver
1. Double SD-15" ultra low distortion woofers
1. Passive or bi-amplified operation
1. Designed for fixed installation and touring
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